This device is OTP memory. It support multiple times of reprogramming task. 
                        Do not suppport single Erase/Blank task. The Partition left size is record to the log.
                        This algo only support .mic format datafile. The mic file contains Config, PMBus LoopA, PMBus LoopB, 
                        FW SVID LoopA, FW SVID LoopB, FW SVID LoopD and Partial PMBus section has been validated. 
                        In case your data file contains more data types, please notice that it has not been validated yet.
                        