Support for STM SPC58 microcontrollers.

Process UTEST OTP area:
  If enabled and the data file contains appropriate records
  the programmer will process the UTEST OTP area. 
  WARNING: 
  Settings in the UTEST area can prevent further access to the device!
  Extreme care must be taken when programming this area!
