This algo will make chip boot from external SD card to program eFuses. eFuses can only program once.By default will implement SD card version check, please fill in the right value to sf OTP Keywriter Version.