Register Definition:
Status Register 1: S7 - S0
	Bit:	Name:								Settings:
	7		Status Register Protection			0: Disabled (Default), 1: Enabled
	6-2		Block Protect Bits					See Protected Area Table

Status Register 2: S15 - S8
	Bit:	Name:								Settings:
	14		Status Register Protection 1		0: Disabled (Default), 1: Enabled
	11		Security Register Lock Bit			0: Unlocked, 1: Locked (OTP)

Configuration Register Byte 1: 7 - 0
	Bit:	Name:								Settings:
	4-0		Dummy Cycle Configuration			Default: 6 (0x06)

	Minimum value for dummy cycle configuration is 3 (0x03), maximum value is 30 (0x1E)

Configuration Register Byte 3: 7 - 0
	Bit:	Name:								Settings:
    7-4		On Die Termination					Default: ODT Disabled (0b1111xxxx)
	3-0		Driver Strength Configuration		Default: 50 Ohm (0xFF)

Configuration Register Byte 4: 7 - 0
	Bit:	Name:								Settings:	
	3		DLP Configuration					Default: DLP Disabled (0bxxxx1xxx)
	2		Protection Configuration			Default: BP Protection (0bxxxxx1xx)

Configuration Register Byte 5: 7 - 0
	Bit:	Name:								Settings:
	0		Beyond 128Mb Address Configuration	0: Enabled, 1: Disabled (Default)

Configuration Register Byte 6: 7 - 0
	Bit:	Name:								Settings:
	0		XIP Configuration					0: Enabled, 1: Disabled (Default)

Configuration Register byte 7: 7 - 0
	Bit:	Name:								Settings:
	1-0		Wrap Configuration					Default: Wrap Disabled (0xFF)