Register definition: 
Status Register 1: S7 - S0
  Bit        Name                              Settings:    
   7         Status Register Protect           0: Disabled(Default), 1: Enabled
  4-2        Block Protection Bits[2:0]        See Protected Area table