Support for NXP S32K3 series microcontrollers.

The size of the memory regions represent the maximum available flash memory.
Limitations apply when HSE is installed.
Avoid accessing the restricted areas, otherwise the operation will fail. 

Process UTEST OTP area:
  If the data file contains appropriate UTEST records the programmer will process the UTEST OTP area. 
  WARNING: 
  Settings in the UTEST area can prevent further access to the device!
  Extreme care must be taken when programming this area!
  Do not read the whole area (may cause bus errors), but single records.

HSE firmware installation supported: load FW-IMG in the region provided for this purpose.

