This support sets up an NXP i.MX6 device.
The following information is required:

  a data file with the fuse settings, start address 0x400, little endian format.
  Example for Intel Hex format:
  if you need to program OTP Bank 0, word 7 with value 0x00000008 then the
  data in the file should look like
  :040470000800000080
  Reserved bits in the eFuse mapping are skipped and not programmed and verified.
  The same applies to addresses in the data file that contain only zeros.

Warning:
  eFuses are One-Time-Programmable!
  Please make sure that the settings are correct, especially for the boot mode and the lock fuses, 
  otherwise the microprocessor may be rendered unusable!
    