Register definition: 
Status Register 1: S7 - S0
  Bit        Name                              Settings:    
   7         Block Protection Locked           0: Unlocked (Default), 1: Locked
   2         Block Protection                  0: Entire Memory array is NOT protected (Default) 1: Entire Memory array is protected

Status Register 2: S7 - S0
  Bit        Name                              Settings:    
   4         Reset Enabled                     0: Disabled (Default), 1: Enabled