
 Important note:
    1.  if the datafile contain data for NONMAIN FLASH(0x41C00000 ~  0x41C001FF) in datafile,
        please aware that some setting would disable the access to device forever.
    2.  for special feature 'Enable Unlock of factory reset', it could reprogram the device which 
        has been protected by the NONMAIN setting or some special datafile.

             Default address map of data file(byte):
             0x00000000  ~ 0x00001FFF  MAIN FLASH
             0x41C00000 ~  0x41C001FF NONMAIN FLASH

             